Microsoft Windows 95
Released by Microsoft in 1995
For 386 or higher based IBM PC compatibles.

This is a 1.44MB floppy disk version. Unlike the DMF (1.7mb) version,
these disks may be written to floppy by a lobotomized USB floppy
drive.

To write these images to a disk, use a disk writing tool such as
WinImage.

For faster installation on real hardware, boot a DOS disk, copy the 
contents of all floppies to a folder on the hard drive such as 
c:\setup, then run SETUP.EXE from that folder.

These images can also be resized for use on 1.2mb disks. 
